EIM Prescreen Result

Nat Kale

Wednesday, June 18, 2014

This is an **automatically generated** review of data submitted to EIM.

## [1] "Z:/batches/results/G1300075/Ebey'sResults2013Q1-3.xls.xml\_1166.csv"

# Data Summary

## Parameters

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Parameter | Units | Matrix | Fraction | Method | Count |
| Dissolved Oxygen-Saturation | % | Water |  | MULTIMETER | 37 |
| Temperature, water | deg C | Water |  | MULTIMETER | 37 |
| Dissolved Oxygen | mg/L | Water |  | MULTIMETER | 37 |
| pH | pH | Water |  | MULTIMETER | 37 |
| Specific Conductivity (at 25 deg C) | uS/cm | Water |  | MULTIMETER | 37 |
| Total Suspended Solids | mg/L | Water | Suspended | SM2540D | 40 |
| Nitrate | mg/L | Water | Dissolved | SM4500NO3F | 40 |
| Ortho-phosphate | mg/L | Water | Dissolved | SM4500P-F | 40 |
| Fecal Coliform | cfu/100mL | Water | Suspended | SM9222D | 43 |
| Stream/River Stage | ft | Water |  | Stage-SG | 7 |
| Turbidity | NTU | Water |  | TURBM | 37 |

## Collection Types

|  |  |  |
| --- | --- | --- |
| Collection Type | Parameter | Count |
| Measurement | Dissolved Oxygen | 37 |
| Measurement | Dissolved Oxygen-Saturation | 37 |
| Sample | Fecal Coliform | 43 |
| Sample | Nitrate | 40 |
| Sample | Ortho-phosphate | 40 |
| Measurement | pH | 37 |
| Measurement | Specific Conductivity (at 25 deg C) | 37 |
| Measurement | Stream/River Stage | 7 |
| Measurement | Temperature, water | 37 |
| Sample | Total Suspended Solids | 40 |
| Measurement | Turbidity | 37 |
| Observation | Unable to measure | 5 |

## Locations

|  |  |
| --- | --- |
| Location | Count |
| ICSP1 | 54 |
| ICSP2 | 57 |
| ICSP3 | 50 |
| ICSP4 | 55 |
| ICSP5 | 65 |
| ICSP6 | 50 |
| ICSP7 | 61 |

# Summary Plots



